**FIX-A-LEAK INSTRUCTIONS**

Fix-a-leak is highly recommended for small leaks that are difficult to detect/repair, which makes it cost effective for older spas that you do not wish to spend a lot of time/money on repairs.

Never use more than one SMALL bottle on a spa at one time. A second application may be required.

As the spa has to be drained and let sit for 48 hours, this project will have to be done in the Spring/Summer.

**INSTRUCTIONS FOR SPA USE**

1. Turn off all jets inside the spa and all diverters (control knobs).
2. Remove the filters, (this a good time to cleanse the filters overnight with the chemical filter cleaner, rinse and let dry before use for fiber pleats to regain natural form – suggested to have a second set to switch every 3 months)
3. Activate the fix-a-leak by continually shaking the bottle for at least 20mins.
4. Hit the jets/pumps to start circulation. Pour entire bottle of the fix-a-leak solution directly into the hole of the filter assembly.
5. Circulate the spa for two full hours, leaving the cover off (after the 15 – 20 run cycle go back to press jet/pump option again – this will have to be done 4-8 times)
6. Let spa run normally on its own 48 hours (you cannot use the spa during this time).
7. Drain spa as normal, important to let spa sit empty for 48 hours.
8. Wipe spa down with vinegar/water solution, refill and add filters and chemicals, as normal.
9. A second bottle application may be required, where the above steps would be followed

Enjoy!!